VkÅu gkWy ds ikl VaªklQkeZj vkfn fo|qr dk;Z

¼o’kZ 2014&15½

gsrq

fufonk izi=

fufonk izi= cspus dh frfFk%&fnukad 10-10-2014 ls 27-10-2014 lka; 1%00 cts rd

fufonk vkaeU=.k dh frfFk%& fnukad 28-10-2014 lka; 3%00 cts rd Vw&fcM ds vk/kkj ij

rduhdh o foRrh; fcM vkaefU=r dh tkrh gSA

fufonk [kksyus dh frfFk fnukad 28-10-2014 lka; 4%00 cts rd rduhdh fcM esa lQy fufonknkrkvksa dh gh foRrh; fcM [kksyh tk;sxhA

fufonk izi= ewY; :0 1000-00++13-50 VSDl

uxj fuxe] nsgjknwu

uxj fuxe] nsgjknwuA

fufonk izi=

:0 1000+13-5 izfr”kr

lfoZl VSDl izfr fufonk

VSfDudy fcM

uxj fuxe ifjlj VkÅu gky ds ikl VªaklQkeZj yxkus vkfn fo|qr dk;Z lEcfU/k

1. ljdkj }kjk ekU;rk izkIr “,” Js.kh ds fo|qr Bsdsnkj dk izek.k i= nsuk gksxkA
2. lsy VSDl uEcj nsuk gksxkA
3. bUde VSDl iSu uaEcj nsuk gksxk@xr nks o’kksZa dk vk;dj fjVuZ Hkh nsuk gksxkA
4. VªaklQkeZj vkbZ0,l0vkbZ0 ekdZ] dkWij okbZfUMxa rFkk ikoj dkiksZjs”ku }kjk Lohd`r dEiuh dk yxkuk gksxk o xkjUVh pkj o’kksZa dh nsuh gksxhA
5. lEiw.kZ dk;Z dh ,d o’kZ rd fu%”kqYd eSUVsusUl djuh gksxhA
6. dsfcy gSoYl] ikSyhdSc] ikbZeu dk yxkuk gksxkA
7. ,e0lh0ch0@,e0lh0lh0ch0 vkfn gSoYl] ,y0 ,.M Vh0 dh yxkuh gksxhA
8. foxr nks o’kksZa dk VuZ vksoj :0 ,d djksM ds fo|qr lEcfU/kr dk;ksZa dk izek.k i= nsuk gksxkA
9. tekur /kujkf”k :0 33000-00 lh0Mh0vkj0@,Q0Mh0vkj0 ys[kkf/kdkjh uxj fuxe nsgjknwu ds uke VsfDudy fcM ds lkFk nsuh vfuok;Z gS] vU;Fkk fufonk ij fopkj ugh fd;k tk;sxkA
10. fujh{kd fo|qr lqj{kk mRrjk[k.M }kjk tkjh Hkkj voeqfDr gsrq djk;s x;s ,p0Vh0 dk;ksZa dh fujh{k.k vk[;k izLrqr djuh gksxhA

vf/k”kklh vfHk;Urk

uxj fuxe] nsgjknwuA

Nagar Nigam, Dehra dun

Fininancial Bid of Construction of Various Plinths for Errection of Transformer & Panel Board.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Sr No | Description | Dimension | Qty | Unit | Rate | Amount. |
| 1 | Excavation work | 1x2.75x2.25x0.30 | 1.86 | Cum |  |  |
| 2.a | PCC work | 2x2.75x0.45x0.075 | 0.19 | Cum |  |  |
| 2.b | PCC work | 2x2.25x0.45x0.075 | 0.15 | Cum |  |  |
| 3.a | Brick Work | 2x2.50x0.90x0.23 | 1.035 | Cum |  |  |
| 3.b | Brick Work | 2x1.54x0.90x0.23 | 0.638 | Cum |  |  |
| 4.a | Plaster | 2x2.50x0.90 | 4.5 | 7 |  |  |
| 4.b | Plaster | 2x2.00x0.90 | 3.6 | Sqm |  |  |
| 5 | Return Earth Filling | 1x1.56x2.04x0.90 | 2.86 | Cum |  |  |
| 6 | RCC | 1x2.5x2x0.15 | 0.75 | Cum |  |  |
| 7.a | TMT Bar 10 sqmm | 26x2x0.60 | 31.35 | Kg |  |  |
| 7.b | TMT Bar 10 sqmm | 21x2.50x0.60 | 31.35 | Kg |  |  |
|  |  |  |  |  |  |  |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Sr No | Description | Dimension | Qty | Unit | Rate | Amount. |
| 1 | Excavation work | 0.90x0.75x0.30 | 0.2 | Cum |  |  |
| 2 | PCC work | 2x0.90x0.45x0.075 | 0.061 | Cum |  |  |
| 3.a | Brick Work | 2x0.750x0.90x0.23 | 0.31 | Cum |  |  |
| 3.b | Brick Work | 2x0.14x0.90x0.23 | 0.06 | Cum |  |  |
| 4 | PCC work | 0.60x0.90x0.15 | 0.0815 | Cum |  |  |
| 4a | Plaster | 2x0.75x0.90 | 1.35 | Sqm |  |  |
| 4b | Plaster | 2x0.60x0.90 | 1.08 | Sqm |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |

vf/k”kklh vfHk;Urk

uxj fuxe] nsgjknwuA

**--2--**

Nagar Nigam, Dehra dun

Fininancial Bid for Leying of XLPE Aromored Cable of Various Size & SITC of Electrical Panel Board.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Sr No | Description | Qty | Unit | Rate | Amount. |
| 1 | Supply & Leying of 11 KV, 3X120 sqmm HT aluminum cable armored, XLPE seathed in trench with brick, sand for coushning. | 10 | Mtr |  |  |
| 2 | Supply & Leying of 1100 V,3.5X120 sqmm aluminum cable Armored, XLPE seathed in trench with brick, sand for coushning. 5101(R)(A) | 100 | Mtr |  |  |
| 3 | Supply & Leying of 1100 V,3.5X70 sqmm aluminum cable Armored, XLPE seathed in trench with brick, sand for coushning. (P) | 210 | Mtr |  |  |
| 4 | Supply & Leying of 1100 V,3.5X50 sqmm aluminum cable Armored, XLPE seathed in trench with brick, sand for coushning. (O) | 110 | Mtr |  |  |
| 5 | Supply & Leying of 1100 V,3.5X50 sqmm aluminum cable Armored, XLPE seathed in trench with brick, sand for coushning. (C) | 100 | Mtr |  |  |
| 6 | HT outdoor joint from 70 to 120 sqmm for HT cable. | 2 | Nos |  |  |
|  |  |  |  |  |  |
|  | **Fabrication of outdoor electrical** |  |  |  |  |
| 1 | Distribution panel borard with MS sheet & powder coated. | 1 | Nos |  |  |
| 1.a | Incoming thermal magnetic & micro proceser release MCCB 4 pol 400 Amp (35k) | 1 | Nos |  |  |
| 1.b | Outgoing thermo magnetic proceser MCCB 4 pole 200 Amp | 1 | Nos |  |  |
| 1.c | Outgoing thermo magnetic proceser MCCB 4 pole 100 Amp | 5 | Nos |  |  |
| 1.d | 4 pole 63 Amp MCCB | 2 | Nos |  |  |
| 1.e | 4 pole single pole MCCB 40 Amp | 4 | Nos |  |  |
| 1.f. | Amp meter, Volt meter with selector switch Supply of factory febriacted, powder coated, | 2 | Set |  |  |
| 2. | MS terminal Box with 200+100 Amps TPN Busbar. Cable End termination of 120 sqmm. | 3 | Nos |  |  |
| 3. | Aluminum armoured XLPE cable with Aluminum Lugs & Cable glands. Cable Eng termination of 70 sqmm. | 2 | Set |  |  |
| 4. | Aluminum armoured XLPE cable with Aluminum Lugs & Cable glands. | 6 | Set |  |  |
| 5. | EARTHING 600x600x6m G.L full earthing | 2 | Nos |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |

vf/k”kklh vfHk;Urk

uxj fuxe] nsgjknwuA

**--3--**

Nagar Nigam, Dehra dun

Fininancial Bid for SITC of 11KV 440 V Transformer.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Sr No | Description | Qty | Unit | Rate | Amount. |
| 1 | Supply, Installation, Testing & Commissioning of 11 KV 250 KVA 11000/440 VoltAC, 3 phase. 3 phase & Nutral LT supply. | 1 | Job |  |  |
| 2 | Supply & Errection of swaged MS Tubular pole 9.5 mtr long, with proper concreting & plinth. | 2 | Nos |  |  |
| 3 | Supply, Installation, Testing & Commissioning of 3 phase, 11 KV Gang Operated Switch, with 3 nos 11 kv fuse set. | 1 | Nos |  |  |
| 4 | S@B of 600X600X6mm G.I Plate vertically forearthing with its top at least 3.5 mtr below ground level. Complete in all respect. | 2 | Nos |  |  |
|  |  |  |  |  |  |

vf/k”kklh vfHk;Urk

uxj fuxe] nsgjknwuA