¼o’kZ 2014&15½

fofHkUu okMksZa esa LVªhV ykbZV iksy ,oa ykbZu yxkus lEcU/kh

gsrq

fufonk izi=

fufonk izi= ewY; :0 5000-00

Iyl 675-00lfoZl VSDl

fufonk izi= cspus dh frfFk%&fnukad 14-10-2014 ls 28-10-2014 lka; 1%00 cts rd

fufonk vkaeU=.k dh frfFk%& fnukad 29-10-2014 lka; 3%00 cts rd Vw&fcM ds vk/kkj ij

rduhdh o foRrh; fcM vkaefU=r dh tkrh gSA

fufonk [kksyus dh frfFk fnukad 29-10-2014 lka; 4%00 cts rduhdh fcM esa lQy fufonknkrkvksa dh gh foRrh; fcM [kksyh tk;sxhA

uxj fuxe] nsgjknwu

Financial/Commercial Bid

Street light at different wards of Nagar Nigam D. Dun.

|  |  |  |  |
| --- | --- | --- | --- |
| Shedule Item No | Item | Rate Per Unit | Amount(IN INR) |
| 7113 | Supply & fixing of street tubular pole 9-00 mts long designated 410 SP-32 in 1:3:6 cement concrete foundation and including excavation back filling etc. and painting with two coat of All Paint over red oxide primer complete in all respects. |  |  |
| 71207123 | Supply & fixing of 75x90 mm Shackle insulator 100x65 mm pin insulator with MS pole clamps including G.I. bolts/ spindle nuts etc. complete with red oxide primer & two coat of synthetic enamel paints etc. complete in all respects. |  |  |
| 7126 | Supply & erection of over head line (Single phase two wire) A.C.S.R weasel conductor on new poles/service bracket including binding stringing etc. complete in all respects. |  |  |
| 7127 | Supply & fixing of G.I wire no 8 running earth on poles/ service bracket including binding etc. complete in all respects. |  |  |
| 7129 | Supply & fixing of stay set at least 3.5 mts away from the poles complete with galvanized 19 mm dia x1.80 mts long stay rod 30 cmx30cmx6.3 mm anchor plate, thimble stay clamp stay insulator 19 mmx600 mm double screw lightener 7/3.15 mm G.I. stay wire etc. in 1:3:6 cement concrete complete in all respects. |  |  |
|  | Supply & burying of G.I rod of 2.5 m long and 20 mm dia. By driving it vertically inside the ground for its full length with top at least 0.6m below the ground level with G.I. wire of 5mm dia, support 16mm dia. 32 mm long G.I. bolt with washer G.I. lug welded to G.I. for earthing etc. complete in all respects. MR |  |  |
|  |  |  |  |

 vf/kd`r izkf/kdkjh@fufonknkrk ds gLrk{kj eksgj lfgr

 uke%& -------------------------------------------------------

 irk%& --------------------------------------------------------

 --------------------------------------------------------

 ---------------------------------------------------------

 Qksu ua0------------------------------------------------------------------

vf/k”kklh vfHk;Urk

uxj fuxe] nsgjknwuA

uxj fuxe] nsgjknwu

VSfDudy fcM

fu;e ,oa “krsZa

1. mRrjk[k.M “kklu fo|qr lqj{kk funs”kky; }kjk , Js.kh esa iathd`r Bsdsnkjksa dk ykbZlsUl ysuk vfuok;Z gksxkA
2. iSu dkMZ ua0 dh izfr ,oa bude VSDl fjVuZ xr rhu o’kksZa dk nsuk vfuok;Z gksxkA
3. :0 nks yk[k dh lh0Mh0vkj0 ys[kkf/kdkjh] uxj fuxe] nsgjknwu ds uke ns; gksxh nsuh vfuok;Z gS] vU;Fkk fufonk ij fopkj ugh fd;k tk;sxkA
4. dk;Z u djus dh n”kk esa f}rh;@r`rh; fufonk nkrk ls U;wure njksa ij dk;Z djk;k tk;sxk] rFkk j{kk/ku tCr dj fn;k tk;sxkA
5. cSysUl “khV xr rhu o’kksZa dk lh0,0 }kjk izekf.kr djds nsuk vfuok;Z gksxk
6. VuZ vksoj :0 1-00 djksM¼,d djksM :i;s½ dk xr rhu o’kksZa dk nsuk vfuok;Z gksxkA
7. fufonk esa yks0fu0fo0 ds lSM~;wy esa nh x;h LisflfQds”ku ds vuqlkj dk;Z djuk gksxkA
8. uxj fuxe nsgjknwu dh lhek ds vUrxZr okMksZa esa iksy ,oa ykbZu vkfn yxkus ds fy;s njsa lHkh dj ,oa dkVsZt lfgr nsuh gksxhA
9. uxj fuxe] nsgjknwu dh lhek esa yxk;s iksy ,oa ykbZu vkfn yxkus ds i”pkr ,d o’kZ dh xkjUVh nsuh gksxhA
10. deZpkfj;ksa ds lqj{kk nq?kZVuk chek@ih0,Q0 vkfn dh ftEesokjh Lo;a fufonk nkrk dh gksxhA
11. j{kk/ku 10 izfr”kr uxj fuxe] nsgjknwu ds uke cU/kad cSad xkjUVh@flD;ksfjVh ds :i esa lQy fufonknkrk dks nsuk gksxkA
12. rduhdh fcM esa lQy djus okyh QeZ dh gh foRrh; fcM [kksyh tk;sxhaA
13. rduhdh fufonk ,oa foRrh; fufonk dks vyx&vyx fyQkQs esa nsuh gksxh] nksuks fyQkQksa dks ,d cMs fyQkQs esa j[ks tk;sxsaA
14. LVªhV ykbZV ykbZu ,oa iksyksa dk fo|qr fujh{kd mRrjk[k.M “kklu nsgjknwu }kjk fujh{k.k mijkUr dk;Z lUrks’k tud izek.k i= ysuk gksxkA

vf/k”kklh vfHk;Urk]

uxj fuxe] nsgjknwuA