dk;kZy; uxj fuxe] nsgjknwuA

fufonk lwpuk

uxj fuxe] nsgjknwu }kjk fuxe ifjlj fLFkr VkÅu gkWy ds fo|qr la;kstu dks mPphd`r djus gsrq 11@0-4 ds0oh0 milaLFkku dk fuekZ.k o ,p0Vh0@,y0Vh0 izksVsDlu fMokbZl vkfn dk;Z djk;s tkus gsrq mRrjk[k.M ds ikoj dkjiksjs”ku@fo|qr lqj{kk funs”kky;@yksd fuekZ.k foHkkx@jkT; vFkok dsUnz ljdkj ds “kkldh;@v)Z”kkldh; foHkkx esa iathd`r Bsdsnkjksa@QeksZ ls fu/kkZfjr izi=ksa ij ßVw&fcMÞ flLVe ij leqfpr :i ls cUn rduhdh o foRrh; fufonk fnukad 26-09-14 dh lka; 3%00 cts rd vkeaf=r dh gSa] mDr fufonk tks fd fnukad 26-09-14 dks gh lka;% 4%00 cts [kksyh tka,xhA dsoy rduhdh fufonk esa mRrh.kZ@vuqeksfnr gksus ij gh foRrh; fufonk ij fopkj fd;k tk,xkA

fufonk izi= uxj fuxe] nsgjknwu ds ekxZ izdk”k vuqHkkx rFkk vf/k”kklh vfHk;Urk d{k esa fnukad 08-09-14 dk;kZy; le; ls fnukad 25-09-14 dks iwokZUg 1%00 cts rd fu/kkZfjr “kqYd tek djk dj izkIr fd, tk ldrs gSaA fufonk izi= osc lkbZV nagarnigamdehradun.com ds uxj fuxe fyad ls Hkh izkIr fd;s tk ldrs gSa rFkk e; fufonk “kqYd ds jftLVMZ Mkd@dksfj;j ls fu/kkZfjr le; ls Hksts tk ldrs gSa@fufonk ckDl esa Mkys tk ldrs gSaA Mkd O;oLFkk esa gq, foyEc ij uxj fuxe mRrjnk;h ugh gksxkA rduhdh fcM ds lkFk j{kk/ku layXu djuk vfuok;Z gSA j{kk/ku ys[kkf/kdkjh] uxj fuxe] nsgjknwu ds uke ca/kd gksxkA fdlh Hkh ;k leLr fufonk dks fcuk dkj.k crk;s fujLr djus dk vf/kdkj eq[; uxj vf/kdkjh uxj fuxe nsgjknwu esa fufgr gksxkA

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| dk;Z dk fooj.k | vkax.ku jkf”k | j{kk/ku | fufonk izi= “kqYd | dk;Z lekfIr vof/k |
| 1. uxj fuxe ifjlj esa 11@0-4 ds0oh0 milLaFkku dk fuekZ.k o ,p0Vh0 izksVSDlu fMokbZl vkfn dk;Z | 11]29942-00 | 33000-00 | 1000+13-5 % lfoZl VSDl | ,d ekg |

eq[; uxj vf/kdkjh

uxj fuxe] nsgjknwuA

bZ&esy- nagarnigam2008@yahoo.com

i=kad%& ------------------------@ekxZ iz0@14&15 fnukad%&------------------------

**izfrfyfi%&** izfrfyfi%&

1. ek0 uxj izeq[k]uxj fuxe] nsgjknwuA
2. lEiknd ------------------------------------------------------- dks bl vuqjks/k ds lkFk izsf’kr gS fd mDr fufonk dks layXu izk:i esa izdkf”kr dj fcy ds lkFk lekpkj i= dh nks izfr;ka fu%”kqYd bl dk;kZy; dks izsf’kr djsaA
3. Jh vrqy oekZ dks bl funsZ”k ds lkFk izsf’kr fd fufonk dks uxj fuxe dh osc lkbV esa viyksM djsaA
4. uxj fuxe uksfVl cksMZ gsrqA

eq[; uxj vf/kdkjh

uxj fuxe] nsgjknwu

VkÅu gkWy ds ikl VaªklQkeZj vkfn fo|qr dk;Z

¼o’kZ 2014&15½

gsrq

fufonk izi=

fufonk izi= ewY; :0 1000-00++13-50 VSDl

uxj fuxe] nsgjknwu

uxj fuxe] nsgjknwuA

fufonk izi=

:0 1000+13-5 izfr”kr

lfoZl VSDl izfr fufonk

VSfDudy fcM

uxj fuxe ifjlj VkÅu gky ds ikl VªaklQkeZj yxkus vkfn fo|qr dk;Z lEcfU/k

1. ljdkj }kjk ekU;rk izkIr “,” Js.kh ds fo|qr Bsdsnkj dk izek.k i= nsuk gksxkA
2. lsy VSDl uEcj nsuk gksxkA
3. bUde VSDl iSu uaEcj nsuk gksxk@xr nks o’kksZa dk vk;dj fjVuZ Hkh nsuk gksxkA
4. VªaklQkeZj vkbZ0,l0vkbZ0 ekdZ] dkWij okbZfUMxa rFkk ikoj dkiksZjs”ku }kjk Lohd`r dEiuh dk yxkuk gksxk o xkjUVh pkj o’kksZa dh nsuh gksxhA
5. lEiw.kZ dk;Z dh ,d o’kZ rd fu%”kqYd eSUVsusUl djuh gksxhA
6. dsfcy gSoYl] ikSyhdSc] ikbZeu dk yxkuk gksxkA
7. ,e0lh0ch0@,e0lh0lh0ch0 vkfn gSoYl] ,y0 ,.M Vh0 dh yxkuh gksxhA
8. foxr nks o’kksZa dk VuZ vksoj :0 ,d djksM ds fo|qr lEcfU/kr dk;ksZa dk izek.k i= nsuk gksxkA
9. tekur /kujkf”k :0 33000-00 lh0Mh0vkj0@,Q0Mh0vkj0 ys[kkf/kdkjh uxj fuxe nsgjknwu ds uke VsfDudy fcM ds lkFk nsuh vfuok;Z gS] vU;Fkk fufonk ij fopkj ugh fd;k tk;sxkA
10. fujh{kd fo|qr lqj{kk mRrjk[k.M }kjk tkjh Hkkj voeqfDr gsrq djk;s x;s ,p0Vh0 dk;ksZa dh fujh{k.k vk[;k izLrqr djuh gksxhA

vf/k”kklh vfHk;Urk

uxj fuxe] nsgjknwuA

Nagar Nigam, Dehra dun

Fininancial Bid of Construction of Various Plinths for Errection of Transformer & Panel Board.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Sr No | Description | Dimension | Qty | Unit | Rate | Amount. |
| 1 | Excavation work | 1x2.75x2.25x0.30 | 1.86 | Cum |  |  |
| 2.a | PCC work | 2x2.75x0.45x0.075 | 0.19 | Cum |  |  |
| 2.b | PCC work | 2x2.25x0.45x0.075 | 0.15 | Cum |  |  |
| 3.a | Brick Work | 2x2.50x0.90x0.23 | 1.035 | Cum |  |  |
| 3.b | Brick Work | 2x1.54x0.90x0.23 | 0.638 | Cum |  |  |
| 4.a | Plaster | 2x2.50x0.90 | 4.5 | 7 |  |  |
| 4.b | Plaster | 2x2.00x0.90 | 3.6 | Sqm |  |  |
| 5 | Return Earth Filling | 1x1.56x2.04x0.90 | 2.86 | Cum |  |  |
| 6 | RCC | 1x2.5x2x0.15 | 0.75 | Cum |  |  |
| 7.a | TMT Bar 10 sqmm | 26x2x0.60 | 31.35 | Kg |  |  |
| 7.b | TMT Bar 10 sqmm | 21x2.50x0.60 | 31.35 | Kg |  |  |
|  |  |  |  |  |  |  |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Sr No | Description | Dimension | Qty | Unit | Rate | Amount. |
| 1 | Excavation work | 0.90x0.75x0.30 | 0.2 | Cum |  |  |
| 2 | PCC work | 2x0.90x0.45x0.075 | 0.061 | Cum |  |  |
| 3.a | Brick Work | 2x0.750x0.90x0.23 | 0.31 | Cum |  |  |
| 3.b | Brick Work | 2x0.14x0.90x0.23 | 0.06 | Cum |  |  |
| 4 | PCC work | 0.60x0.90x0.15 | 0.0815 | Cum |  |  |
| 4a | Plaster | 2x0.75x0.90 | 1.35 | Sqm |  |  |
| 4b | Plaster | 2x0.60x0.90 | 1.08 | Sqm |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |

vf/k”kklh vfHk;Urk

uxj fuxe] nsgjknwuA

**--2--**

Nagar Nigam, Dehra dun

Fininancial Bid for Leying of XLPE Aromored Cable of Various Size & SITC of Electrical Panel Board.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Sr No | Description | Qty | Unit | Rate | Amount. |
| 1 | Supply & Leying of 11 KV, 3X120 sqmm HT aluminum cable armored, XLPE seathed in trench with brick, sand for coushning. | 10 | Mtr |  |  |
| 2 | Supply & Leying of 1100 V,3.5X120 sqmm aluminum cable Armored, XLPE seathed in trench with brick, sand for coushning. 5101(R)(A) | 100 | Mtr |  |  |
| 3 | Supply & Leying of 1100 V,3.5X70 sqmm aluminum cable Armored, XLPE seathed in trench with brick, sand for coushning. (P) | 210 | Mtr |  |  |
| 4 | Supply & Leying of 1100 V,3.5X50 sqmm aluminum cable Armored, XLPE seathed in trench with brick, sand for coushning. (O) | 110 | Mtr |  |  |
| 5 | Supply & Leying of 1100 V,3.5X50 sqmm aluminum cable Armored, XLPE seathed in trench with brick, sand for coushning. (C) | 100 | Mtr |  |  |
| 6 | HT outdoor joint from 70 to 120 sqmm for HT cable. | 2 | Nos |  |  |
|  |  |  |  |  |  |
|  | **Fabrication of outdoor electrical** |  |  |  |  |
| 1 | Distribution panel borard with MS sheet & powder coated. | 1 | Nos |  |  |
| 1.a | Incoming thermal magnetic & micro proceser release MCCB 4 pol 400 Amp (35k) | 1 | Nos |  |  |
| 1.b | Outgoing thermo magnetic proceser MCCB 4 pole 200 Amp | 1 | Nos |  |  |
| 1.c | Outgoing thermo magnetic proceser MCCB 4 pole 100 Amp | 5 | Nos |  |  |
| 1.d | 4 pole 63 Amp MCCB | 2 | Nos |  |  |
| 1.e | 4 pole single pole MCCB 40 Amp | 4 | Nos |  |  |
| 1.f. | Amp meter, Volt meter with selector switch Supply of factory febriacted, powder coated, | 2 | Set |  |  |
| 2. | MS terminal Box with 200+100 Amps TPN Busbar. Cable End termination of 120 sqmm. | 3 | Nos |  |  |
| 3. | Aluminum armoured XLPE cable with Aluminum Lugs & Cable glands. Cable Eng termination of 70 sqmm. | 2 | Set |  |  |
| 4. | Aluminum armoured XLPE cable with Aluminum Lugs & Cable glands. | 6 | Set |  |  |
| 5. | EARTHING 600x600x6m G.L full earthing | 2 | Nos |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |

vf/k”kklh vfHk;Urk

uxj fuxe] nsgjknwuA

**--3--**

Nagar Nigam, Dehra dun

Fininancial Bid for SITC of 11KV 440 V Transformer.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Sr No | Description | Qty | Unit | Rate | Amount. |
| 1 | Supply, Installation, Testing & Commissioning of 11 KV 250 KVA 11000/440 VoltAC, 3 phase. 3 phase & Nutral LT supply. | 1 | Job |  |  |
| 2 | Supply & Errection of swaged MS Tubular pole 9.5 mtr long, with proper concreting & plinth. | 2 | Nos |  |  |
| 3 | Supply, Installation, Testing & Commissioning of 3 phase, 11 KV Gang Operated Switch, with 3 nos 11 kv fuse set. | 1 | Nos |  |  |
| 4 | S@B of 600X600X6mm G.I Plate vertically forearthing with its top at least 3.5 mtr below ground level. Complete in all respect. | 2 | Nos |  |  |
|  |  |  |  |  |  |

vf/k”kklh vfHk;Urk

uxj fuxe] nsgjknwuA